%! TEX root = ../thesis.tex
\thispagestyle{empty}

\begin{center}
    {\bfseries Abstract}
\end{center}
\begin{abstract}~\\
    %Accurate measurements and voltage supply is a integral part for any system to work perfectly.
    The PowerIts main purpose is to measure and supply different voltages.
    In the Human Brain Projects BrainScaleS system, it delivers power to all system components.
    This thesis will provide a calibration of the PowerIt board as well as a regulation mechanism for its 1.8V power supplies.

    Calibration of this board, will provide more accurate measurements, and allow for later regulation of its 1.8V outputs.
    First its circuitry will be examined and their behavior tested.
    Then the circuits can be calibrated.
    With these calibrations a method for regulating the main analog and digital power supplies will be implemented and verified on the Power wafer. 

    This thesis also contains the changes done to the PowerIt firmware while working on these tasks.
    The new firmware now has a new protocol for communication over a I\(^2\)C connection.
    It can be used for accessing any calibration parameter or on board measurement.
\end{abstract}
\vspace{1cm}
\begin{center}
    {\bfseries Zusammenfassung}
\end{center}
\begin{abstract}~\\
    Die Hauptaufgabe des PowerIts ist die Messung von, und Versorgung mit, verschiedenen Spannungen, die im BrainScaleS System des Humen Brain Projekts ben\"{o}tigt werden.
    
    Diese Arbeit liefert eine Kalibration des PowerIt, sowie eine Methode zur Regelung der \SI{1.8}{\volt} Spannungsausg\"{a}nge.
    Zuerst werden daf\"{u}r die verbauten Schaltungen untersucht, auf ihr verhalten getestet und daraus Kalibrationsdaten erfasst.
    Die sp\"{a}tere Regulierung der haupt Analog- und Digitalspannungen h\"{a}ngt dabei von der vorausgegangenen Kalibrierung ab.

    Zus\"{a}tzlich enth\"{a}llt diese Arbeit die \"{A}nderungen, die an der Firmware vorgenommen worden sind, w\"{a}hrend diese Aufgaben bearbeitet wurden.
    Die neue Firmware enth\"{a}llt nun ein neues Protokoll f\"{u}r die Kommunikation \"{u}ber einen I\(^2\)C-Bus.
    Dieses Protokoll kann dazu genutzt werden auf beliebige Kalibrationsdaten oder Messwerde zuzugreifen.
\end{abstract}